

The displacement spectrum of the PT407 (with bellows) cryostat when both the pulse tube engine and the bellows separated sleeve are supported directly on the ground.

Fig 6