

Figure 7 PT407 (without bellows) placed on the ground. Note the increased noise relative to Figure 6 PT407 (with bellows). Note also that the horizontal displacement spectrum is larger than the vertical . The high frequency vertical spectrum became corrupted due to a bad spot on the floppy disk and is not included

in the figures.